**附件5仿真文件格式要求**

**Annex 5 Format Requirements of Simulation Files**

**要求各投标单位提供仿真相关技术资料：**

**Relevant simulation technology materials required to provide by each bidder:**

一、要求各投标单位提供2009版或2010版3dmax模型原始文件和相贴图材质、同时提供每栋建筑的四个立面效果图格式为JPG，像素在5000左右、每个方案的总平面格式为JPG，像素在5000左右。


I. Each bidder shall provide original documents of 3DMAX model (2009 or 2010 version) and the materials of relevant textures, and meanwhile, provide the rendering drawings in the format of JPG of four elevations of every building, with pixel of around 5000. The general plan of each scheme is JPG, with pixel of around 5000.

二、提供简化模型，包括各建筑立面纹理和总平面图的简化模型,简化模型不能共面，建筑总面数在100到10000面之间。

II. Provide simplified models, including the simplified models of elevation texture and general plan of each building. No co-plane is allowed for simplified models, and total building planes shall be of from 100 to 10000.

**附：模型简化示意图：**

**Attachment: Schematic diagram of model**



原复杂模型简化的模型立面纹理需提供的用于（几十万个面）（几十个面）（原来模型渲染生成）仿真制做的模型

The elevation texture of the models simplified from original complicated models shall provide for the simulated models (of hundreds of thousands of planes) (tens of planes) (generated from the rendering of original models).